Search Tips

Search is based on keyword.

`Ex: "Procedures"`

Do not search with natural language

`Ex: "How do I write a new procedure?"`

Give Feedback Support Portal

# Inputs

O_DisparityToDepth has the following inputs:

Camera | A pre-tracked Nuke stereo camera that describes the camera setup that is used to shoot the Source images. This can be a camera you have tracked with the CameraTracker node or imported to Nuke from a third-party camera tracking application. In Nuke, a stereo camera can be either: • a single Camera node in which some or all of the controls are split, or • two Camera nodes (one for each view) followed by a JoinViews node (Views > JoinViews). The JoinViews node combines the two cameras into a single output.
A single Camera node with split controls. | Two cameras combined using Nuke’s JoinViews node.
Disparity | A stereo pair of images. O_DisparityToDepth requires upstream disparity vectors. If they do not already exist, insert an O_DisparityGenerator node after the image sequence to calculate them. See DisparityGenerator for more information.

To see a table listing the nodes or channels each Ocula node requires in its inputs, see Node Dependencies.