Search Tips

Search is based on keyword.

`Ex: "Procedures"`

Do not search with natural language

`Ex: "How do I write a new procedure?"`

Give Feedback Support Portal

# Inputs

O_NewView has the following inputs:

CleanPlate | A clean background plate used to fill areas of occlusion when Correction is set to Use CleanPlate. Note: If no image is connected, a Channels missing at CleanPlate input. Please connect RGB input to CleanPlate error is displayed.
Source | A stereo pair of images. If disparity channels are not embedded in the images, you need to add an O_DisparityGenerator node after the image sequence. O_NewView also requires an occlusion mask, which you can generate using an O_OcclusionDetector node.

To see a table listing the nodes or channels each Ocula node requires in its inputs, see Node Dependencies.