Search Tips

Search is based on keyword.

`Ex: "Procedures"`

Do not search with natural language

`Ex: "How do I write a new procedure?"`

Give Feedback Support Portal

# Inputs

O_InteraxialShifter has the following inputs:

Source | A stereo pair of images. If disparity channels and occlusion masks are not embedded in the images, you need to insert an O_DisparityGenerator and an O_OcclusionDetector node after the image sequence.

To see a table listing the nodes or channels each Ocula node requires in its inputs, see Node Dependencies.